layers : 2
minimum trace width : >=10 mil
minimum trace spacing : >=10 mil
minimum drill size : 0.4 mm
width : 361 mm
height : 203.5 mm

Gerber Files:
https://github.com/marekl123/atari800xl

Platinenservice
https://www.pcbway.com/project/shareproject/Atari_800XL_PCB_remake_v1_1.html

Projekt-Blog:
https://ezcontents.org/atari-800xl-pcb-remake
https://ezcontents.org/atari-800xl-bill-materials-bom
https://ezcontents.org/atari-800xl-pcb-soldering-and-troubleshooting

